IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView_V2.0]"
File name: "demo250hp.ifc"
Time stamp: "2026-02-27T02:39:44"
Preprocessor: "IFC Toolkit 2.0.5.0"
Originating system: "Advance Steel 2026"
Application: "Advance Steel" version "2026" identifier "Autodesk.Advance Steel" by Organization "Autodesk"

People and organizations
  Person (no name given) of Organization (no name given)
  Owner history of Person (no name given) of Organization (no name given) | application "Advance Steel" version "2026" identifier "Autodesk.Advance Steel" by Organization "Autodesk" | state READWRITE | change ADDED | created 1772159984 (2026-02-27T02:39:44Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT
  IFCSITE "Site"
    IFCBUILDING "Estrutura 1"
      IFCBUILDINGSTOREY "Default Storey" | elevation 0.
        contains 3 elements
          1 x IFCBEAM | object type "-" | names: "-" | descriptions: "HP 250x62.0(H)" | material: "S235JRG2" | property sets: Pset_BeamCommon, ProfileProperties
          2 x IFCPLATE | object type "-" | names: "-" | descriptions: "-" | material: layers "A36" ("A36" 10.) | property sets: Pset_PlateCommon

Property sets
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "indefinido" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 1500. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  ProfileProperties | properties | on 1 object (1 IFCBEAM)
    Section = "HP 250x62.0(H)" (IFCIDENTIFIER)
    SectionFamily = "Gerdau W" (IFCIDENTIFIER)
  Pset_PlateCommon | properties | on 2 objects (2 IFCPLATE)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "indefinido" (IFCIDENTIFIER)
    ThermalTransmittance (no value)